(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6062)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "${PCB_NAME}")
		(date "${CURRENT_DATE}")
		(rev "${PCB_VERSION}")
	)
	(layers
		(0 "F.Cu" mixed)
		(4 "In1.Cu" power)
		(6 "In2.Cu" power)
		(2 "B.Cu" mixed)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.2104)
				(material "Prepreg")
				(epsilon_r 4.4)
				(loss_tangent 0.025)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.065)
				(material "FR4-Core")
				(epsilon_r 4.6)
				(loss_tangent 0.025)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.2104)
				(material "Prepreg")
				(epsilon_r 4.4)
				(loss_tangent 0.025)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
	)
	(embedded_files
		(file
			(name LED_0402_1005Metric.step)
			(type model)
		)
		(file
			(name R_0402_1005Metric.step)
			(type model)
		)
	)
	(property "PCB_NAME" "blinky")
	(property "PCB_VERSION" "v0.0.0")
	(property "PCB_GIT_HASH" "d10d3c0")
	(footprint "kicad_libraries_kicad-footprints_Resistor_SMD@9.0.3:R_0402_1005Metric"
		(layer "F.Cu")
		(at 148.3825 104.01)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "ERJ-2RKF1001X"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/RDA0000/AOA0000C304.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Path" "R1.R"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Mpn" "ERJ-2RKF1001X"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Package" "0402"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Prefix" "R"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Resistance" "1k"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Type" "resistor"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VCC")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LED_ANODE")
		)
		(embedded_fonts no)
		(model "kicad-embed://R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(embedded_files
			(file
				(name R_0402_1005Metric.step)
				(type model)
			)
		)
	)
	(footprint "kicad_libraries_kicad-footprints_LED_SMD@9.0.3:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 148.6175 105)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "VLMS1500-GS08"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.vishay.com/docs/82554/vlmo1500.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED RED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Path" "D1.LED"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Color" "red"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Semiconductor Opto Division"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Mpn" "VLMS1500-GS08"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Package" "0402"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Prefix" "D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Type" "led"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LED_ANODE")
		)
		(embedded_fonts no)
		(model "kicad-embed://LED_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(embedded_files
			(file
				(name LED_0402_1005Metric.step)
				(type model)
			)
		)
	)
	(embedded_fonts no)
)
